#
SUSPENSION SPECIFICATIONS

BME020001013102

## Wheel and Tire

### Standard tire

European (L.H.D. U.K.) specs.

Item | Specification
--- | ---
Tire | Size | 205/65R15 94T | 215/60R16 95H
Wheel | Size | 15 × 6J | 15 × 6JJ | 16 × 6 1/2J
Material | Aluminum alloy | Steel | Steel, Aluminum alloy
Offset | (mm {in}) | 50 {1.97}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

Australian, General (L.H.D. R.H.D.) specs.

Item | Specification
--- | ---
Tire | Size | 205/65R15 94H | 215/60R16 95H | 215/60R17 96H
Wheel | Size | 15 × 6J | 15 × 6JJ | 16 × 6 1/2J | 17 × 7J
Material | Aluminum alloy | Steel | Aluminum alloy
Offset | (mm {in}) | 50 {1.97}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

### Temporary spare tire

European (L.H.D. U.K.) specs.

Item | Specification
--- | ---
Tire | Size | T135/90D15 | T145/80D16
Wheel | Size | 15 × 4T | 16 × 4T
Material | Steel
Offset | (mm {in}) | 45 {1.77}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

Australian, General (L.H.D. R.H.D.) specs.

Item | Specification
--- | ---
Tire | Size | T135/90D15 | T145/80D16
Wheel | Size | 15 × 4T | 16 × 4T
Material | Steel
Offset | (mm {in}) | 35 {1.38} | 45 {1.77}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}