#
ON-BOARD DIAGNOSTIC TEST [AJ]

BME010200102208

## DTCs Reading Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector located the left side (L.H.D.) or right side (R.H.D.) of the center console.

3. Retrieve DTCs by WDS or equivalent.

## Pending trouble code access procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector located the left side (L.H.D.) or right side (R.H.D.) of the center console.

3. Retrieve PENDING TROUBLE CODES by WDS or equivalent.

## Freeze frame PID data access procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector located the left side (L.H.D.) or right side (R.H.D.) of the center console.

3. Record the FREEZE FRAME DATA by WDS or equivalent.

## On-Board system readiness tests access procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector located the left side (L.H.D.) or right side (R.H.D.) of the center console.

3. Monitor the OBD systems operating status by WDS or equivalent.

## Diagnostic monitoring test results access procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector located the left side (L.H.D.) or right side (R.H.D.) of the center console.

3. Access to the DIAGNOSTIC MONITORING TEST RESULTS and read the test results by WDS or equivalent.