#
SCHEDULED MAINTENANCE

BME000000013201

## For Europe (L.H.D. U.K.)

Chart symbols:

I: Inspect: Inspect and clean, repair, adjust, or replace if necessary.

R: Replace

C: Clean

Remarks:

• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation. All inspections and adjustments must be made by an expert repairer, we recommend an Authorized Mazda Repairer. • After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.
*1: | If the vehicle is operated under any of the following conditions, change the engine oil and oil filter every 10,000 km {6,250 miles} or shorter.
| a. Driving in dusty conditions. b. Extended periods of idling or low speed operation. c. Driving for long period in cold temperatures or driving regularly at short distance only.
*2: | Also inspect and adjust the power steering and air conditioner drive belts, if installed.
*3: | If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, change the brake fluid annually.
*4: | If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
*5: | Replacement of the timing belt is required at every 100,000 km {62,500 miles}. Failure to replace the timing belt may result in damage to the engine.
*6: | Replacement of the timing belt is required at every 120,000 km {75,000 miles}. Failure to replace the timing belt may result in damage to the engine.

Maintenance Item | Maintenance Interval (Number of months or kilometers (miles), whichever comes first)
--- | ---
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108
×1000 km | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180
×1000 miles | 12.5 | 25 | 37.5 | 50 | 62.5 | 75 | 87.5 | 100 | 112.5
GASOLINE ENGINE
Engine valve clearance | Audible inspect every 120,000km (75,000miles), if noisy, adjust
Spark plugs | Replace every 100,000 km (62,500 miles)
Air cleaner element*4 |  |  | R |  |  | R |  |  | R
Evaporative system (if installed) |  |  | I |  |  | I |  |  | I
DIESEL ENGINE
Engine valve clearance | I |  |  |  |  | I |  |  |
Engine timing belt | Finland, Sweden, Norway*5 | Replace every 100,000 km (62,500 miles)
Others*6 | Replace every 120,000 km (75,000 miles)
Fuel filter |  |  | R |  |  | R |  |  | R
Fuel injection system | I |  | I |  |  | I |  |  | I
Air cleaner element*4 | C | C | R | C | C | R | C | C | R
E.G.R.system |  |  | I |  |  | I |  |  | I
GASOLINE and DIESEL ENGINE
Engine oil*1 | R | R | R | R | R | R | R | R | R
Engine oil filter*1 | R | R | R | R | R | R | R | R | R
Drive belts*2 |  |  | I |  |  | I |  |  | I
Cooling system (Including coolant level adjustment) |  | I |  | I |  | I |  | I |
Engine coolant | Replace at first 4 years or 100,000 km (62,500 miles); after that, every 2 years
Fuel lines and hoses |  | I |  | I |  | I |  | I |
Battery electrolyte level and specific gravity | I | I | I | I | I | I | I | I | I
Brake fluid*3 |  | R |  | R |  | R |  | R |
Brake lines, hoses and connections | I | I | I | I | I | I | I | I | I
Parking brake | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses | I | I | I | I | I | I | I | I | I
Disc brakes | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |
Manual transmission/transaxle oil |  |  |  |  | R |  |  |  |
Front and rear suspension and ball joints |  | I |  | I |  | I |  | I |
Drive shaft dust boots |  | I |  | I |  | I |  | I |
Exhaust system and heat shields | Inspect every 80,000km (50,000miles) or 60 months
Cabin air filter (if installed) (pollen filter) |  | R |  | R |  | R |  | R |
Body condition (for rust, corrosion and perforation) | Inspect annually
Tires (including spare tire) (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I

## For Israel

Chart symbols:

I: Inspect: Inspect and clean, repair, adjust, or replace if necessary.

R: Replace

C: Clean

Remarks:

• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation. All inspections and adjustments must be made by an Authorized Mazda Dealer. • After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.
*1: | If the vehicle is operated under any of the following conditions, change the engine oil and oil filter every 10,000 km {6,250 miles} or shorter.
| a. Driving in dusty conditions. b. Extended periods of idling or low speed operation. c. Driving for long period in cold temperatures or driving regularly at short distance only.
*2: | Also inspect and adjust the power steering and air conditioner drive belts, if installed.
*3: | If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, change the brake fluid annually.
*4: | If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
*5: | This is a full function check of electrical systems such as lights, wiper and washer systems (including wiper blades), and power windows.

Maintenance Item | Maintenance Interval (Number of months or kilometers (miles), whichever comes first)
--- | ---
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120 | 132 | 144
×1000 Km | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120 | 135 | 150 | 165 | 180
×1000 Miles | 9 | 18 | 27 | 36 | 45 | 54 | 63 | 72 | 81 | 90 | 99 | 108
Drive belts*2 | I | I | I | I | I | I | I | I | I | I | I | I
Engine oil*1 | R | R | R | R | R | R | R | R | R | R | R | R
Engine oil filter*1 | R | R | R | R | R | R | R | R | R | R | R | R
Cooling system (Including coolant level adjustment) |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | Replace at first 4 years or 90,000km (54,000 miles); after that, every 2 years
Air cleaner element*4 | C | C | C | R | C | C | C | R | C | C | C | R
Fuel filter | Replace every 105,000 km (63,000 miles)
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I
Spark plugs | Replace every 90,000 km (54,000 miles)
Evaporative system |  |  |  | I |  |  |  | I |  |  |  | I
Battery electrolyte level and specific gravity | I | I | I | I | I | I | I | I | I | I | I | I
Brake lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I
Brake fluid*3 | I | R | I | R | I | R | I | R | I | R | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses | I | I | I | I | I | I | I | I | I | I | I | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |  | I |  | I
Automatic transmission/transaxle fluid level |  | I |  | I |  | I |  | I |  | I |  | I
Front and rear suspension and ball joints |  |  | I |  | I |  | I |  | I |  | I |
Drive shaft dust boots |  |  | I |  | I |  | I |  | I |  | I |
Exhaust system and heat shields | Inspect every 75,000km (45,000miles)
Cabin air filter (if installed) | R | R | R | R | R | R | R | R | R | R | R | R
Body condition (for rust, corrosion and perforation) | Inspect annually
All electrical system*5 | I | I | I | I | I | I | I | I | I | I | I | I
Tires (including spare tire) (with inflation pressure adjustment) | I | I | I | I | I | I | I | I | I | I | I | I

## For General (L.H.D. R.H.D)

Chart symbols:

I: Inspect: Inspect and clean, repair, adjust, or replace if necessary.

R: Replace

T: Tighten

C: Clean

Remarks:

• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation. All inspections and adjustments must be made by an Authorized Mazda Dealer. • After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.
*1: | If the vehicle is operated under any of the following conditions, change the engine oil and oil filter more often than recommended intervals.
| a. Driving in dusty conditions. b. Extended periods of idling or low speed operation. c. Driving for long period in cold temperatures or driving regularly at short distance only.
*2: | Also inspect and adjust the power steering and air conditioner drive belts, if installed.
*3: | If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, change the brake fluid annually.
*4: | If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
*5: | This is a full function check of electrical systems such as lights, wiper and washer systems (including wiper blades), and power windows.

Maintenance Item | Maintenance Interval (Number of months or kilometers (miles), whichever comes first)
--- | ---
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
×1000 Km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 | 140 | 150 | 160
×1000 Miles | 6.25 | 12.5 | 18.75 | 25 | 31.25 | 37.5 | 43.75 | 50 | 56.25 | 62.5 | 68.75 | 75 | 81.25 | 87.5 | 93.75 | 100
Engine valve clearance (for L3 engine) | Audible inspect every 120,000km (75,000miles), if noisy, adjust
Drive belts*2 | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Engine oil*1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Engine oil filter*1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | Replace every 2 years
Air cleaner element*4 |  | C |  | C |  | R |  | C |  | C |  | R |  | C |  | C
Spark plugs | Replace every 100,000 km (62,500 miles)
Fuel filter |  |  |  | R |  |  |  | R |  |  |  | R |  |  |  | R
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Evaporative system (if installed) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Battery electrolyte level and specific gravity |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake lines, hoses and connections |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake fluid*3 | I | I | I | R | I | I | I | R | I | I | I | R | I | I | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Drum brakes |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Manual transmission/transaxle oil |  |  |  |  |  |  |  |  |  | R |  |  |  |  |  |
Automatic transmission/transaxle fluid level |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Front and rear suspension and ball joints |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Drive shaft dust boots |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Exhaust system and heat shields | Inspect every 80,000km (50,000miles)
Bolts and nuts on chassis and body |  | T |  | T |  | T |  | T |  | T |  | T |  | T |  | T
All electrical system*5 |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Body condition (for rust, corrosion and perforation) | Inspect annually
Cabin air filter (if installed) |  | R |  | R |  | R |  | R |  | R |  | R |  | R |  | R
Tires (including spare tire) (with inflation pressure adjustment) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I

## For Australia

Chart symbols:

I: Inspect: Inspect and clean, repair, adjust, or replace if necessary.

R: Replace

T: Tighten

C: Clean

Remarks:

• The ignition and fuel systems are highly important to the emission control system and to efficient engine operation. All inspections and adjustments must be made by an Authorized Mazda Dealer. • After the prescribed period, continue to follow the described maintenance at the recommended intervals.
• Refer below for a description of items marked* in the maintenance chart.
*1: | If the vehicle is operated under any of the following conditions, change the engine oil and oil filter more often than recommended intervals.
| a. Driving in dusty conditions. b. Extended periods of idling or low speed operation. c. Driving for long period in cold temperatures or driving regularly at short distance only.
*2: | Also inspect and adjust the power steering and air conditioner drive belts, if installed.
*3: | If the brakes are used extensively (for example, continuous hard driving or mountain driving) or if the vehicle is operated in extremely humid climates, change the brake fluid annually.
*4: | If the vehicle is operated in very dusty or sandy areas, clean and if necessary, replace the air cleaner element more often than the recommended intervals.
*5: | This is a full function check of electrical systems such as lights, wiper and washer systems (including wiper blades), and power windows.

Maintenance Item | Maintenance Interval (Number of months or km, whichever comes first)
--- | ---
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60 | 66 | 72 | 78 | 84 | 90 | 96
×1000 Km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 | 140 | 150 | 160
Engine oil | *1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Engine oil filter | *1 | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R | R
Drive belts | *2 | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Spark plugs | Replace every 100,000 km
Fuel filter |  |  |  |  |  | R |  |  |  |  |  | R |  |  |  |
Fuel lines and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Air cleaner element | *4 |  |  | C |  |  | R |  |  | C |  |  | R |  |  | C |
Cooling system |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Engine coolant | Replace at first 4years or 80,000 km; after that, every 2years
Evaporative system (if installed) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Battery electrolyte level and specific gravity |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake lines, hoses and connections |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Brake fluid | *3 | I | I | I | R | I | I | I | R | I | I | I | R | I | I | I | R
Parking brake | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power brake unit (Brake booster) and hoses |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Disc brakes | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Power steering fluid, lines, hoses and connections | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I | I
Steering operation and linkages |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Automatic transmission/transaxle fluid level |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Front and rear suspension and ball joints |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Driveshaft dust boots |  |  |  | I |  |  |  | I |  |  |  | I |  |  |  | I
Exhaust system and heat shields | Inspect every 80,000km
Tires (including spare tire) (with inflation pressure adjustment) |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I
Bolts and nuts on chassis and body |  | T |  | T |  | T |  | T |  | T |  | T |  | T |  | T
All electrical system | *5 |  | I |  | I |  | I |  | I |  | I |  | I |  | I |  | I

## Scheduled Maintenance Service (Specific Work Required)

### For Europe (L.H.D. U.K.)

Bold frame: New item

Maintenance Item | Specific Work Required
--- | ---
ENGINE
Engine valve clearance | Measure clearance.
Drive belts | Inspect for wear, cracks and fraying, and check tension. Replace drive belt.
Engine timing belt | Replace engine timing belt.
Engine oil | Replace engine oil and inspect for leakage.
Engine oil filter | Replace oil filter and inspect for leakage.
COOLING SYSTEM
Cooling system (including coolant level adjustment) | Check coolant level and quality, and inspect for leakage.
Engine coolant | Replace coolant.
FUEL SYSTEM
Air cleaner element | Inspect for dirt, oil and damage. Clean air cleaner element (by blowing air). Replace air cleaner element.
Fuel filter | Replace fuel filter.
Fuel lines and hoses | Inspect for cracks, leakage and loose connection.
Fuel injection system | Update to injection amount correction with WDS. (See W/M)
IGNITION SYSTEM
Spark plugs | Inspect for wear, damage, carbon, high-tension lead condition and measure plug gap. Replace spark plugs.
EMISSION CONTROL SYSTEM
Evaporative system | Check system operation (see W/M), vapor lines, vacuum fitting hoses and connection.
E.G.R. system | Check system operation (see W/M), vacuum fitting hoses and connection.
ELECTRICAL SYSTEM
Battery electrolyte level and specific gravity | Check level and specific gravity.
CHASSIS and BODY
Brake fluid | Check fluid level and inspect for leakage. Replace brake fluid.
Brake lines, hoses and connections | Inspect for cracks, damage, chafing, corrosion, scars, swelling and fluid leakage.
Parking brake | Check lever stroke.
Power brake unit (Brake booster) and hoses | Check vacuum lines, connections and check valve for improper attachment, air tightness, cracks chafing and deterioration.
Disc brakes | Test for judder and noise. Inspect caliper for correct operation and fluid leakage, brake pads for wear. Check disc plate condition and thickness.
Power steering fluid, lines, hoses and connections | Check fluid level and condition. Inspect for loose connection, routing, damage, and leaks.
Steering operation and linkages | Check steering wheel free play, hard steering, and operation noise. Check linkages, boots and ball joints condition. Check grease or gear oil.
Front and rear suspension and ball joints | Inspect for grease leakage, cracks, damage and looseness.
Manual transmission/transaxle oil | Check oil level and inspect for leakage. Replace manual transmission/transaxle oil.
Drive shaft dust boots | Inspect for grease leakage, cracks, damage and looseness.
Body condition (for rust, corrosion and perforation) | Inspect body surface for paint damage, rust, corrosion and perforation.
Exhaust system and heat shields | Inspect for damage, corrosion, looseness of connections and gas leakage.
Tires (including spare tire) (with inflation pressure adjustment) | Check air pressure and inspect tires for tread wear, damage and cracks; and wheels for damage and corrosion.
AIR CONDITIONER SYSTEM
Cabin air filter | Replace cabin air filter.