#
POWER OUTSIDE MIRROR INSPECTION

BME091269110202

1. Remove the front door trim.

2. Partially peel off the door screen.

3. Disconnect the power outside mirror connector.

4. Apply battery positive voltage to the power outside mirror terminals and inspect the operation of the power outside mirror.

  • If not as specified, replace the power outside mirror.

Terminal | Mirror operation
--- | ---
B+ | GND
B | D | Up
D | B | Down
F | D | Left
D | F | Right

5. Inspect for continuity between the power outside mirror terminals.

  • If not as specified, replace the power outside mirror.