#
PARAMETER IDENTIFICATION (PID) DATA MONITORING FUNCTION [FN4A-EL]

BME050200000T07
• The PID mode allows access to certain data values, analog and digital input and output, calculations and system state information.

## Monitor Item Table

Display on the tester | Definition | Unit/Condition | PCM terminal
--- | --- | --- | ---
GEAR | Gear commanded by module | 1/2/3/4 | 3P, 3S, 4Y, 4AB, 4AC
LINEDES | Target line pressure | kPa | inHg | 3V, 3Y
LPS | Pressure control solenoid control signal in PCM | mA | 3V, 3Y
OP SW B | Oil pressure switch | ON/OFF | 3T
SSA/SS1 | Shift solenoid A control signal in PCM | % | 4AB
SSB/SS2 | Shift solenoid B control signal in PCM | % | 4AC
SSC/SS3 | Shift solenoid C control signal in PCM | % | 4Y
TCS | HOLD switch | ON/OFF | 3Q
TFT | ATF temperature | °C | °F | 3D
TFTV | ATF temperature signal voltage | V | 3D
THOP | TP sensor | % | 2A
TP | TP signal in PCM | % | 2A
TP signal voltage | V | 2A
TR | Transaxle range | P/R/N/D/S/L | 1W, 3E, 3H, 3K, 3N
TSS | Input/turbine speed | rpm | 3G, 3J
VPWR | Battery positive voltage | V | 2Y, 2Z
VSS | Vehicle speed | km/h | mph | 3C