#
STARTING PROCEDURE FOR ON-BOARD DIAGNOSTIC TEST MODE

BME090266900201

  Note

  • All DTCs displayed in the on-board diagnostic test mode should be entered in the Audio Repair Order Form.

1. Turn the ignition switch to the ACC or ON position.

2. First press the POWER button, then simultaneously press the AM button and CLOCK button for 2 seconds or more.

1 | AM button
2 | CLOCK button
3 | SEEK button (with RDS)
4 | SEEK button (without RDS)
5 | POWER button (with RDS)
6 | POWER button (without RDS)

  Note

  • If several DTCs are in the memory, they can be displayed by the SEEK button.

3. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.