#
UNDERBODY FLAT-PLANE DIMENSIONS

BME098053010B01

.

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Crossmember No.1 standard hole | ø10 {0.40}
B | Front side frame standard hole | ø16 {0.63}
C | Front suspension mounting block surface hole center | ø98 {3.86}
D | Front suspension mounting bolt | M12 {0.47}
E | Front suspension mounting bolt | M14 {0.55}
F | Front B frame standard hole | 20×24 {0.79×0.94}
G | Front B frame standard hole | ø20 {0.79}
H | Rear side frame standard hole | ø16 {0.63}
I | Stopper bracket standard hole | ø10 {0.40}
J | Rear side frame standard hole | ø16 {0.63}
K | Rear side frame standard hole | 16×20 {0.63×0.79}
L | Trailing arm mounting hole | ø12 {0.47}