#
NO.27 HOLD indicator light ILLUMINATE WHEN HOLD SWITCH IS NOT TURNED TO ON [JA5A-EL]

BME050301030263

27 | HOLD indicator light illuminate when HOLD switch is not turned to ON
DESCRIPTION | • HOLD indicator light in instrument cluster illuminate even though the HOLD switch turned off with the ignition switch at ON.
POSSIBLE CAUSE | • HOLD switch or related wiring harness malfunction.

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Inspect the TCS PID value using the WDS or equivalent. Is the TCS PID value normal? | Yes | Inspect for short to GND circuit in following harness. HOLD indicator light in instrument cluster and TCM terminal E including instrument cluster circuit board
No | Inspect the HOLD switch. (See HOLD SWITCH INSPECTION [JA5A-EL].) If the HOLD switch normal, inspect for short to ground circuit between the HOLD switch terminal and TCM terminal 2I.
2 | • Verify the test results.

  - If normal, return to the diagnostic index to service any additional symptoms.
  - If the malfunction remains, inspect the related Service Bulletins and/or On-line Repair Information and perform repair or diagnosis.

  • If the vehicle is repaired, troubleshooting is completed.
  • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.