#
DTC 22

BME010266350205

DTC 22 | Cruise control switch (RESUME/ACCEL switch)
DETECTION CONDITION | • Resistance detected between cruise actuator connector terminal J and ground is other than 68 ohms.
POSSIBLE CAUSE | • Cruise actuator malfunction • Cruise control switch malfunction

Diagnostic procedure

INSPECTION | ACTION
--- | ---
INSPECT CRUISE CONTROL SWITCH • Inspect cruise control switch. (See CRUISE CONTROL SWITCH INSPECTION) • Is cruise control switch okay? | Yes | • Replace cruise actuator. (See CRUISE ACTUATOR REMOVAL/INSTALLATION)
No | • Replace cruise control switch. (See AUDIO CONTROL SWITCH REMOVAL/INSTALLATION)