#
DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION

BME081057010W01

  Warning

  • Handling the air bag module improperly can accidentally deploy the air bag module, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before handling the air bag module. (See SERVICE WARNINGS.)

1. Turn the ignition switch to LOCK position.

2. Disconnect the negative battery cable and wait for more than 1 minute.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. Turn the ignition switch to ON position.

6. Verify that the air bag system warning light illuminates for approximately 6 seconds and then goes off.

  • If the air bag system warning light does not operate in the manner described above, there are malfunctions in the system. Inspect the system using the on-board diagnostic.

1 | Bolt
2 | Connector (See Connector Installation Note.)
3 | Driver-side air bag module

## Connector Installation Note

• Install the connector as shown in the figure.