#
SIMULATION TEST [L3]

BME010200000T06
• The simulation test items for the fuel and emission control systems are as shown in the table below.

Simulation item table

×: Applied
-: Not applied

Simulation item | Applicable component | Operation | Test condition | PCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
ACCS | A/C relay | ON or OFF | × | × | 4O
ALTF | Generator field coil control duty value | ON or OFF | - | × | 1AD
ARPMDES | Desired RPM |  | × | × | -
EVAPCP | Purge solenoid valve | For purge solenoid valve: Actuated by any duty value (0-100%) | × | × | 4U
FAN DUTY | Fan control module | Actuated by any duty value (0-100%) | × | × | 1U
FP | Fuel pump relay | ON or OFF | × | × | 4P*2, 4Q*1
FUELPW1 | Fuel injection duration | Actuated +50%- -50% fuel injection time | - | × | 4W, 4Z, 4AA, 4AD
GENVDSD | Generator voltage desired |  | - | × | -
HTR11 | Front heated exhaust gas oxygen sensor heater | ON or OFF | × | × | 4A
HTR12 | Rear heated exhaust gas oxygen sensor heater | ON or OFF | × | × | 4D
IAC | Idle air control | Actuated by any duty value (0-100%) | × | × | 4G, 4J
IMRC | Variable tumble control solenoid control signal in PCM | ON or OFF | × | × | 4T
IMTV | Variable intake-air system (VIS) solenoid control signal in PCM | ON or OFF | × | × | 4R
INJ#1 | Fuel injector (Cylinder No.1) | ON or OFF | - | × | 4Z
INJ#2 | Fuel injector (Cylinder No.2) | ON or OFF | - | × | 4W
INJ#3 | Fuel injector (Cylinder No.3) | ON or OFF | - | × | 4AD
INJ#4 | Fuel injector (Cylinder No.4) | ON or OFF | - | × | 4AA
SEGRP | EGR valve (stepping motor) | Actuated by any stepping value (0-60 steps) | × | × | 4E, 4H, 4K, 4N
TEST | TEN terminal | ON or OFF | × | × | 1I*3, 1L*4

  *1 :
With immobilizer system
  *2 :
Without immobilizer system
  *3 :
MTX models
  *4 :
ATX models