#
FLASHER UNIT REMOVAL/INSTALLATION

BME091866830W01

  Note

  • Because the lock section of the unit is damaged easily, do not remove the unit from the bracket unless replacement is necessary. Always perform an inspection of the flasher unit before removal.

1. Disconnect the negative battery cable.

2. Remove the bracket.

3. Disconnect the flasher unit connector.

4. Remove the flasher unit by prying the lock section of the upper part with a flathead screwdriver.

5. Install in the reverse order of removal.