#
SYMPTOM TROUBLESHOOTING ITEM TABLE [JA5A-EL]

BME050301030235
• Use the chart below to verify the symptoms of the trouble in order to diagnose the appropriate area.

No. | TROUBLESHOOTING ITEM | DESCRIPTION | PAGE
--- | --- | --- | ---
1 | Vehicle does not move in D, S, L ranges, or in R position | Vehicle does not move when accelerator pedal is depressed. | (See NO.1 VEHICLE DOES NOT MOVE IN D, S, L RANGES, OR IN R POSITION [JA5A-EL].)
2 | Vehicle moves in N position | Vehicle creeps in N position. Vehicle creeps if brake pedal is not depressed in N position. | (See NO.2 VEHICLE MOVES IN N POSITION [JA5A-EL].)
3 | Vehicle moves in P position, or parking gear does not disengage when P is disengaged | Vehicle rolls on a downward slope in P position. Tires are locked when P position is disengaged. Vehicle does not move in D, S, L ranges and R position when the accelerator pedal is depressed, and the engine remains in a stalled condition. | (See NO.3 VEHICLE MOVES IN P POSITION, OR PARKING GEAR DOES NOT DISENGAGE WHEN P IS DISENGAGED [JA5A-EL].)
4 | Excessive creep | Vehicle accelerates in D, S, L ranges and R position when accelerator pedal is not depressed. | (See NO.4 EXCESSIVE CREEP [JA5A-EL].)
5 | No creep at all | Vehicle does not move in D, S, L ranges, or R position when idling on flat paved road. | (See NO.5 NO CREEP AT ALL [JA5A-EL].)
6 | Low maximum speed and poor acceleration | Vehicle acceleration is poor at start. Delayed acceleration when accelerator pedal is depressed while driving. | (See NO.6 LOW MAXIMUM SPEED AND POOR ACCELERATION [JA5A-EL].)
7 | No shifting | Single shift range only. Sometimes shifts correctly. | (See NO.7 NO SHIFTING [JA5A-EL].)
8 | Does not shift to 5GR | Vehicle does not upshift from 4GR to 5GR even though vehicle speed is increased. Vehicle does not shift to 5GR even though accelerator pedal is released in D range at 60 km/h {37 mph}. | (See NO.8 DOES NOT SHIFT TO 5GR [JA5A-EL].)
9 | Abnormal shifting | Shifts incorrectly (incorrect shift pattern). | (See NO.9 ABNORMAL SHIFTING [JA5A-EL].)
10 | Frequent shifting | Downshifting occurs suddenly even when accelerator pedal is depressed slightly in D, S, L ranges except HOLD mode. | (See NO.10 FREQUENT SHIFTING [JA5A-EL].)
11 | Shift point is high or low | Shift point considerably different from automatic shift diagram. Shift delays when accelerating. Shift occurs quickly when accelerating and engine speed does not increase. | (See NO.11 SHIFT POINT IS HIGH OR LOW [JA5A-EL].)
12 | Torque converter clutch (TCC) non-operation | TCC does not operate when vehicle reaches TCC operation range. | (See NO.12 TORQUE CONVERTER CLUTCH (TCC) NON-OPERATION [JA5A-EL].)
13 | No kickdown | Does not downshift when accelerator pedal is fully depressed within kickdown range. | (See NO.13 NO KICKDOWN [JA5A-EL].)
14 | Engine flares up or slips when upshifting or downshifting | When the accelerator pedal is depressed, engine speed increases normally but vehicle speed increase slowly. When the accelerator pedal is depressed while driving, engine speed increases but vehicle speed does not. | (See NO.14 ENGINE FLARES UP OR SLIPS WHEN UPSHIFTING OR DOWNSHIFTING [JA5A-EL].)
15 | Engine flares up or slips when accelerating the vehicle | Engine flares up when the accelerator pedal is depressed for upshifting. Engine flares up suddenly when the accelerator pedal is depressed for downshifting. | (See NO.15 ENGINE FLARES UP OR SLIPS WHEN ACCELERATING VEHICLE [JA5A-EL].)
16 | Judder upon torque converter clutch (TCC) operation | Vehicle jolts when TCC is engaged. | (See NO.16 JUDDER UPON TORQUE CONVERTER CLUTCH (TCC) OPERATION [JA5A-EL].)
17 | Excessive shift shock from N to D or N to R position/range | Strong shock is felt when shifting from N to D or N to R position/range at idle. | (See NO.17 EXCESSIVE SHIFT SHOCK FROM N TO D OR N TO R POSITION/RANGE [JA5A-EL].)
18 | Excessive shift shock is felt when upshifting and downshifting | Excessive shift shock is felt when depressing the accelerator pedal at upshifting. During cruising, excessive shift shock is felt when depressing the accelerator pedal at downshifting. | (See NO.18 EXCESSIVE SHIFT SHOCK IS FELT WHEN UPSHIFTING AND DOWNSHIFTING [JA5A-EL].)
19 | Excessive shift shock on torque converter clutch (TCC) | Strong shock is felt when the TCC engaged. | (See NO.19 EXCESSIVE SHIFT SHOCK ON TORQUE CONVERTER CLUTCH (TCC) [JA5A-EL].)
20 | Noise occurs at idle when vehicle is stopped in all positions/ranges | Transaxle is noisy in all positions and ranges when the vehicle idling. | (See NO.20 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN ALL POSITIONS/RANGES [JA5A-EL].)
21 | Noise occurs at idle when vehicle is stopped in D, S, L ranges, or in R position | Transaxle is noisy in driving ranges when vehicle idling. | (See NO.21 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN D, S, L RANGES, OR IN R POSITION [JA5A-EL].)
22 | No engine braking in L range | Engine speed drops to idle but vehicle coasts when accelerator pedal is released during cruising at medium to high speeds. Engine speed drops to idle but vehicle coasts when accelerator pedal is released when in L range at low vehicle speed. | (See NO.22 NO ENGINE BRAKING IN L RANGE [JA5A-EL].)
23 | Transaxle overheats | Burnt smell emitted from transaxle. Smoke is emitted from transaxle. | (See NO.23 TRANSAXLE OVERHEATS [JA5A-EL].)
24 | Engine stalls when shifted to D, S, L ranges, or in R position | Engine stalls when shifting from N or P position to D, S, L ranges, or R position at idle. | (See NO.24 ENGINE STALLS WHEN SHIFTED TO D, S, L RANGES, OR IN R POSITION [JA5A-EL].)
25 | Engine stalls when driving at slow speeds or stopping | Engine stalls when brake pedal is depressed while driving at low speed or stopping. | (See NO.25 ENGINE STALLS WHEN DRIVING AT SLOW SPEED OR STOPPING [JA5A-EL].)
26 | HOLD indicator light does not illuminate when HOLD switch is turned to on | HOLD indicator light in instrument cluster does not illuminate when the HOLD switch is turned on with the ignition switch at ON. | (See NO.26 HOLD INDICATOR LIGHT DOES NOT ILLUMINATE WHEN HOLD SWITCH IS TURNED TO ON [JA5A-EL].)
27 | HOLD indicator light illuminate when HOLD switch is not turned to on | HOLD indicator light in instrument cluster illuminate even though the HOLD switch turned off with the ignition switch at ON. | (See NO.27 HOLD indicator light ILLUMINATE WHEN HOLD SWITCH IS NOT TURNED TO ON [JA5A-EL].)