#
CONTROL DEVICES AND MONITORING SYSTEM RELATIONSHIP CHART [AJ]

BME010200000T09
×: Applicable

Component |  |  |  |  |  |
--- | --- | --- | --- | --- | --- | ---
Input
Refrigerant pressure switch, A/C switch, blower fan switch and A/C amplifier |  |  |  |  |  | ×
PSP switch |  |  |  |  |  | ×
CKP sensor | × | × | × | × | × | ×
CMP sensor | × | × | × | × | × | ×
VSS | × | × | × | × |  | ×
MAF sensor | × | × | × | × | × | ×
ECT sensor | × | × | × | × | × | ×
IAT sensor | × | × | × | × |  | ×
TP sensor | × | × | × | × |  | ×
EGR boost sensor |  |  |  |  |  | ×
Rear HO2S | × |  |  | × | × |
Front HO2S | × |  | × | × | × |
Output
DLC-2 in driver compartment (Terminal KLN) | × | × | × | × | × | ×
MIL | × | × | × | × | × | ×
Purge solenoid valve |  |  | × | × |  |
EGR valve |  |  |  |  |  | ×
EGR boost sensor solenoid valve |  |  |  |  |  | ×
Fuel injectors |  |  | × |  |  |

  *1 :
European (L.H.D.) specs.
  *2 :
Australian, General (L.H.D. R.H.D.) specs