#
STEERING TECHNICAL DATA

BME065000000W01

Item | Specification
--- | ---
L3 | MZR-CD (RF Turbo)
ENGINE SPEED SENSING POWER STEERING
Steering wheel | Play | (mm {in}) | 0-30 {0-1.18}
Effort | (N·m {kgf·cm, in·lbf}) | 7.8 {80, 69} max.
Steering shaft | Length | (mm {in}) | 847.9-851.9 {33.4-33.5}
Steering gear | Tie-rod end | Rotation torque | (N·m {kgf·cm, in·lbf}) | 0.4-2.5 {3.5-26.0, 3.1-22.5}
[Pull scale reading] | (N {kgf, lbf}) | 3.4-25.5 {0.35-2.60, 0.8-5.7}
Tie rod | Swinging torque | (N·m {kgf·cm, in·lbf}) | 0.1-2.9 {1-30, 0.9-26.0}
[Pull scale reading] | (N {kgf, lbf}) | 0.6-15.4 {0.06-1.58, 0.2-3.47}
Steering rack | Maximum Runout | Large diameter portion | 0.15 {0.006}
(mm {in}) | Small diameter portion | 0.20 {0.008}
Pinion shaft | Rotation torque | (N·m {kgf·cm, in·lbf}) | 0.8-1.3 {8-14, 7-12}
[Pull scale reading] | (N {kgf, lbf}) | 7.9-13 {0.8-1.4, 1.8-3.0}
Gear housing fluid pressure | (MPa {kgf/cm2, psi}) | 8.23-8.92 {84.0-90.9, 1,200-1,290} | 8.64-9.13 {88.2-93.1, 1,260-1,320}
Power steering oil pump | Oil pump fluid pressure | (MPa {kgf/cm2, psi}) | 8.23-8.92 {84.0-90.9, 1,200-1,290} | 8.64-9.13 {88.2-93.1, 1,260-1,320}
Power steering system | Fluid | Type | ATF M-III or equivalent (e.g. DexronII)
Capacity (Approx. quantity) | L.H.D.: 1.09 {1.15, 0.96} R.H.D.: 1.04 {1.10, 0.92} | L.H.D.: 0.96 {1.01, 0.84} R.H.D.: 0.90 {0.95, 0.79}
(L {US qt, Imp qt})