#
NEUTRAL SWITCH INSPECTION [MZR-CD (RF Turbo)]

BME014017640W02

  Note

  • Perform the following test only when directed.

## Continuity Inspection

1. Inspect for continuity between the neutral switch terminals using an ohmmeter.

  • If the neutral switch is okay, but the CPP/PNP PID is out of specification, perform the "Circuit Open/Short Inspection"
  • If not as specified, replace the neutral switch.

Specification

## Circuit Open/Short Inspection

1. Inspect for open/short circuit in the following wiring harnesses.

  • If there is open/short circuit, repair or replace wiring harnesses.

### Open circuit

  • Signal circuit
  - Neutral switch terminal A and PCM terminal 56
  • GND circuit
  - Neutral switch terminal B and GND

### Short circuit

  • Signal circuit
  - Neutral switch terminal A and PCM terminal 56 to GND