#
DTC TABLE [MZR-CD (RF Turbo)]

BME010200000W21
×: Applicable -: Not applicable

DTC | Condition | MIL | Memory function | Page
--- | --- | --- | --- | ---
P0016 | Crankshaft position-camshaft position correlation malfunction | × | × | (See DTC P0016 [MZR-CD (RF Turbo)])
P0088 | Fuel pressure system too high | - | × | (See DTC P0088 [MZR-CD (RF Turbo)])
P0091 | Suction control valve circuit low input | × | × | (See DTC P0091 [MZR-CD (RF Turbo)])
P0092 | Suction control valve circuit high input | × | × | (See DTC P0092 [MZR-CD (RF Turbo)])
P0093 | Fuel system leak detection | × | × | (See DTC P0093 [MZR-CD (RF Turbo)])
P0097 | IAT sensor No.1 circuit low input | × | × | (See DTC P0097 [MZR-CD (RF Turbo)])
P0098 | IAT sensor No.1 circuit high input | × | × | (See DTC P0098 [MZR-CD (RF Turbo)])
P0102 | MAF sensor circuit low input | × | × | (See DTC P0102 [MZR-CD (RF Turbo)])
P0103 | MAF sensor circuit high input | × | × | (See DTC P0103 [MZR-CD (RF Turbo)])
P0107 | Boost sensor circuit low input | × | × | (See DTC P0107 [MZR-CD (RF Turbo)])
P0108 | Boost sensor circuit high input | × | × | (See DTC P0108 [MZR-CD (RF Turbo)])
P0112 | IAT sensor No.2 circuit low input | × | × | (See DTC P0112 [MZR-CD (RF Turbo)])
P0113 | IAT sensor No.2 circuit high input | × | × | (See DTC P0113 [MZR-CD (RF Turbo)])
P0117 | ECT sensor circuit low input | × | × | (See DTC P0117 [MZR-CD (RF Turbo)])
P0118 | ECT sensor circuit high input | × | × | (See DTC P0118 [MZR-CD (RF Turbo)])
P0121 | Accelerator position sensor No.1 circuit performance problem | × | × | (See DTC P0121 [MZR-CD (RF Turbo)])
P0122 | Accelerator position sensor No.1 circuit low input | × | × | (See DTC P0122 [MZR-CD (RF Turbo)])
P0123 | Accelerator position sensor No.1 circuit high input | × | × | (See DTC P0123 [MZR-CD (RF Turbo)])
P0182 | Fuel temperature sensor circuit low input | × | × | (See DTC P0182 [MZR-CD (RF Turbo)])
P0183 | Fuel temperature sensor circuit high input | × | × | (See DTC P0183 [MZR-CD (RF Turbo)])
P0191 | Fuel pressure sensor circuit performance problem | × | × | (See DTC P0191 [MZR-CD (RF Turbo)])
P0192 | Fuel pressure sensor circuit low input | × | × | (See DTC P0192 [MZR-CD (RF Turbo)])
P0193 | Fuel pressure sensor circuit high input | × | × | (See DTC P0193 [MZR-CD (RF Turbo)])
P0200 | Fuel injector circuit malfunction | × | × | (See DTC P0200 [MZR-CD (RF Turbo)])
P0221 | Accelerator position sensor No.2 circuit performance problem | × | × | (See DTC P0221 [MZR-CD (RF Turbo)])
P0222 | Accelerator position sensor No.2 circuit low input | × | × | (See DTC P0222 [MZR-CD (RF Turbo)])
P0223 | Accelerator position sensor No.2 circuit high input | × | × | (See DTC P0223 [MZR-CD (RF Turbo)])
P0300 | Random misfire detection | × | × | (See DTC P0300 [MZR-CD (RF Turbo)])
P0336 | CKP sensor circuit performance problem | × | × | (See DTC P0336 [MZR-CD (RF Turbo)])
P0337 | CKP sensor circuit low input | × | × | (See DTC P0337 [MZR-CD (RF Turbo)])
P0341 | CMP sensor circuit performance problem | × | × | (See DTC P0341 [MZR-CD (RF Turbo)])
P0342 | CMP sensor circuit low input | × | × | (See DTC P0342 [MZR-CD (RF Turbo)])
P0380 | Glow plug relay circuit malfunction | × | × | (See DTC P0380 [MZR-CD (RF Turbo)])
P0500 | VSS circuit malfunction | × | × | (See DTC P0500 [MZR-CD (RF Turbo)])
P0510 | Idle switch circuit malfunction | × | × | (See DTC P0510 [MZR-CD (RF Turbo)])
P0512 | Engine switch circuit malfunction | × | × | (See DTC P0512 [MZR-CD (RF Turbo)])
P0606 | PCM malfunction | × | × | (See DTC P0606 [MZR-CD (RF Turbo)])
P0661 | VSC solenoid valve circuit low input | - | × | (See DTC P0661 [MZR-CD (RF Turbo)])
P0662 | VSC solenoid valve circuit high input | - | × | (See DTC P0662 [MZR-CD (RF Turbo)])
P0850 | Neutral switch circuit malfunction | × | × | (See DTC P0850 [MZR-CD (RF Turbo)])
P1190 | Calibration resistor circuit malfunction | × | × | (See DTC P1190 [MZR-CD (RF Turbo)])
P1602 | Immobilizer unit-PCM communication error | - | × | (See DTC P1602 [MZR-CD (RF Turbo)])
P1603 | Key ID number unregistered in PCM | - | × | (See DTC P1603 [MZR-CD (RF Turbo)])
P1604 | Code word unregistered in PCM | - | × | (See DTC P1604 [MZR-CD (RF Turbo)])
P1621 | Code words do not match after engine cranking | - | × | (See DTC P1621 [MZR-CD (RF Turbo)])
P1622 | Key ID number mismatch | - | × | (See DTC P1622 [MZR-CD (RF Turbo)])
P1623 | Cord word or key ID number read/write error in PCM | - | × | (See DTC P1623 [MZR-CD (RF Turbo)])
P1624 | Immobilizer system communication counter = 0 | - | × | (See DTC P1624 [MZR-CD (RF Turbo)])
P2228 | BARO sensor circuit low input | × | × | (See DTC P2228 [MZR-CD (RF Turbo)])
P2229 | BARO sensor circuit high input | × | × | (See DTC P2229 [MZR-CD (RF Turbo)])