#
THIRD-ROW SEAT REMOVAL/INSTALLATION

BME09135730X201

## Seat

1. Remove the headrests.

2. Remove the bolt. (LH)

3. Stow the third-row seat.

4. Open the cover (LH)

5. Remove the bolts and then remove the third-row seat.

6. Install in the reverse order of removal.

## Hinge

1. Remove the third-row seat.

2. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

3. Remove the third-row seat belt lower anchor.

4. Remove in the order indicated in the table.

1 | Hinge cover
2 | Hinge

5. Install in the reverse order of removal.

## Striker

1. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

2. Remove the nuts and then remove the striker.

3. Install in the reverse order of removal.