#
DTC TABLE

BME090267000202

DTC | Output pattern | Description | Page
--- | --- | --- | ---
1 |  | ID number unregistered in immobilizer unit is input after engine cranking. | DTC 1
2 |  | ID number format error (voltage range, frequency) | DTC 2
3 |  | ID number is not input into immobilizer unit after cranking engine. | DTC 3
11 |  | Coil or wiring harness between immobilizer unit and coil is open circuit. | DTC 11
21 |  | Code word/ID number memorized in immobilizer unit EEPROM cannot be read. | DTC 21
24 |  | Open or short circuit in wiring harness between immobilizer unit and PCM. | DTC 24
30 |  | Immobilizer unit-PCM communication error | DTC 30

  Note

  • Perform the following if the security light stays on:

  - If gasoline engine stalls, go to symptom troubleshooting NO.11 "ENGINE STALLS/QUITS, ENGINE RUNS ROUGH, MISSES, BUCK/JERK, HESITATION/STUMBLE, SURGES" in. (See NO.11 ENGINE STALLS/QUITS, ENGINE RUNS ROUGH, MISSES, BUCK/JERK, HESITATION/STUMBLE, SURGES [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See NO.11 ENGINE STALLS/QUITS, ENGINE RUNS ROUGH, MISSES, BUCK/JERK, HESITATION/STUMBLE, SURGES [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
  - If gasoline engine won't start, go to symptom troubleshooting NO.6 "CRANKS NORMALLY BUT WILL NOT START" in. (See NO.6 CRANKS NORMALLY BUT WILL NOT START [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)) (See NO.6 CRANKS NORMALLY BUT WILL NOT START [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)))
  - If engine condition is normal but light stays on, inspect for continuity between the following wiring harness and body ground: security light and immobilizer unit connector terminal M. Repair or replace the wiring harness.