#
DTC P0182 [MZR-CD (RF Turbo)]

BME010200100W33

DTC P0182 | Fuel temperature sensor circuit low input
--- | ---
DETECTION CONDITION | • PCM monitors input voltage from fuel temperature sensor while engine is running. If input voltage from fuel temperature sensor is below 0.1 V, PCM determines fuel temperature sensor circuit low input.
POSSIBLE CAUSE | • Fuel temperature sensor malfunction • Connector or terminal malfunction • Short to GND in wiring between fuel temperature sensor terminal A and PCM terminal 35 • Fuel temperature sensor signal and GND circuits short each other • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to next step.
No | Go to next step.
2 | INSPECT POOR CONNECTION OF FUEL TEMPERATURE SENSOR CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to Step 7.
No | Go to next step.
3 | INSPECT FUEL TEMPERATURE SENSOR SIGNAL CIRCUIT FOR SHORT TO GND • Turn engine switch to OFF. • Inspect continuity between fuel temperature sensor terminal A and body GND. • Is there continuity? | Yes | Repair or replace harness for short to GND, go to Step 7.
No | Go to next step.
4 | INSPECT FUEL TEMPERATURE SENSOR CIRCUIT FOR SHORT WITH EACH OTHER • Turn engine switch to OFF. • Inspect continuity between fuel temperature sensor terminals A and B. • Is there continuity? | Yes | Repair or replace harness for short with each other, go to Step 7.
No | Go to next step.
5 | INSPECT FUEL TEMPERATURE SENSOR • Inspect fuel temperature sensor. (See FUEL TEMPERATURE SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Repair supply pump, go to Step 7. (See SUPPLY PUMP INSPECTION [MZR-CD (RF Turbo)].)
No | Go to next step.
6 | INSPECT POOR CONNECTION OF PCM CONNECTOR • Turn engine switch to OFF. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace suspected terminal, go to next step.
No | Go to next step.
7 | VERIFY TROUBLESHOOTING OF DTC P0182 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear DTC from PCM memory using WDS or equivalent. • Start engine. • Is same DTC present? | Yes | Replace PCM, go to next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].) • Is there any DTC present? | Yes | Go to applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.