#
AUTOMATIC WINDOW RETURN FUNCTION INSPECTION

BME091259560203

  Warning

  • Do not put your hand, arm, or any part of your body in the window while inspecting. A malfunction in the automatic window return function could cause injury. Be careful not to allow your body to get caught in the window.

  Note

  • The automatic window return function is used only for the driver-side front door.
  • The automatic window return function operates during auto close operation or when the window is closed manually with the IG OFF timer.

1. Fully lower the door glass.

2. Position the handle of the hammer as shown in the figure.

3. Operate the power window switch to the auto close position and close the window.

4. Verify that the window reverses operation when it contacts the handle of the hammer and that it opens approximately 200 mm {7.87 in}.

  • If not as specified, inspect the system following the TROUBLESHOOTING [POWER WINDOW SYSTEM].