#
DTC 07 ERR10 OR 07:ER10

BME090266900211

DTC 07 ERR10 or 07:Er10 | MD player-base unit communication line
DETECTION CONDITION | • Base unit detects communication error with MD player
POSSIBLE CAUSE | • Malfunction of connectors between base unit and MD player • MD player malfunction • Base unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CONNECTOR • Remove MD player and inspect connector for the following.

  - Deformation of pin
  - Poor connection of female terminal
  - Pinching of foreign material

• Is connector okay?
Yes
Go to next step.
No | Repair connector, then go to next step.
2 | VERIFY THAT MD PLAYER IS INSTALLED WITH BASE UNIT • Install MD player and verify its installation condition. • Is MD player securely installed? | Yes | Go to next step.
No | Securely install MD player, then go to next step.
3 | INSPECT MD PLAYER • Clear DTC. • Turn ignition switch to ACC or ON position and hold for 3 seconds or more. • Start on-board diagnostic test mode. • Is DTC 07 ERR10 or 07:Er10 displayed? | Yes | Replace base unit and MD player.
No | Troubleshooting completed.