#
SIMULATION FUNCTION [FN4A-EL]

BME050219090108

• By using the WDS or equivalent, simulation items for input/output parts preset in the PCM can be optionally selected and operated regardless of PCM control conditions.

## Simulation Item Table

X: Available

Simulation item | Applicable component | Unit/Condition | Operation | PCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
LPS | Pressure control solenoid control signal in PCM | % | X | N/A | 3V, 3Y
SSA/SS1 | Shift solenoid A control signal in PCM | % | X | N/A | 4AB
SSB/SS2 | Shift solenoid B control signal in PCM | % | X | N/A | 4AC
SSC/SS3 | Shift solenoid C control signal in PCM | % | X | N/A | 4Y