#
SERVICE PRECAUTIONS

BME000000000B02

## Arrangement of Workshop

• Arrangement of the workshop is important for safe and efficient work.

## Safety Precautions

• Protective head covering and safety shoes should always be worn. Depending upon the nature of the work, gloves, safety glasses, ear protectors, face shield, etc., should also be used.

## Vehicle Protection

• Use seat covers and floor covers.
• Use heat-resistant protective covers to protect glass areas and seats from heat or sparks during welding.
• Protect items such as moldings, garnishes, and ornaments with tape when welding.

## Remove Dangerous Articles

• Remove the fuel tank before using an open flame in that area. Plug connection piping to prevent fuel leakage.

## Use of Pulling Equipment

• When using pulling equipment, keep away from the pulling area and use safety wires to prevent accidents.

## Prevent Short Circuits

• Turn the ignition switch to the LOCK position.
• Disconnect the battery cables.

• Securely connect the welding machine ground near the welding area.