#
DTC P0506 [L3]

BME010200500W03

DTC P0506 | Idle control system RPM lower than expected
--- | ---
DETECTION CONDITION | • Actual idle speed is lower than expected by 100 rpm for 14 s, when brake pedal is depressed (brake switch is on) and steering wheel is held straight ahead (power steering pressure switch is off).

  Note

  • If atmospheric pressure is less than 72.3 kPa {542 mmHg, 21.3 inHg} or intake air temperature is below -10 °C {14 °F}, PCM cancels diagnosis of P0506.

Diagnostic support note
• This is a continuous monitor (CCM).
• MIL illuminates if PCM detects the above malfunction conditions in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• PENDING CODE is available if PCM detects the above malfunction condition during first drive cycle.
• FREEZE FRAME DATA is available.
• DTC is stored in PCM memory.
POSSIBLE CAUSE | • IAC valve malfunction • Air cleaner element clogged • Air intake passage clogged • A/C relay control circuit malfunction • Generator malfunction
• Purge solenoid valve malfunction
• Low engine compression (Over capacity of blow-by gas)
• PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to next step.
No | Record FREEZE FRAME DATA on repair order, then go to next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Check for related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to available Service Information. • If vehicle is not repaired, go to next step.
No | Go to next step.
3 | VERIFY RELATED PENDING OR STORED DTCS • Turn ignition key to OFF, then ON (Engine OFF). • Verify pending code or stored DTCs using WDS or equivalent. • Is any other DTC present? | Yes | Repair applicable DTCs. (See DTC TABLE [L3].)
No | Go to next step.
4 | INSPECT IAC VALVE MALFUNCTION • Perform IAC valve inspection. (See IDLE AIR CONTROL (IAC) VALVE INSPECTION [L3].) • Is IAC valve okay? | Yes | Go to next step.
No | Replace IAC valve, then go to Step 11.
5 | INSPECT A/C MAGNET CLUTCH OPERATION • Turn blower motor switch off. • Is magnet clutch still on? | Yes | Go to "A/C IS ALWAYS ON OR A/C COMPRESSOR RUNS CONTINUOUSLY." of ENGINE SYMPTOM TROUBLESHOOTING then go to step 11. (See NO.24 A/C IS ALWAYS ON OR A/C COMPRESSOR RUNS CONTINUOUSLY [L3].)
No | Go to next step.
6 | INSPECT PURGE SOLENOID VALVE MALFUNCTION • Perform purge solenoid valve inspection. (See PURGE SOLENOID VALVE INSPECTION [L3].) • Is purge solenoid valve okay? | Yes | Go to next step.
No | Replace purge solenoid valve, then go to Step 11.
7 | INSPECT AIR CLEANER ELEMENT • Remove air cleaner element with engine running. • Does engine speed increase? | Yes | Replace air cleaner element, then go to Step 11.
No | Go to next step.
8 | INSPECT THROTTLE BODY PASSAGE • Is throttle body clogged? | Yes | Clean or replace throttle body passage, then go to Step 11.
No | Go to next step.
9 | INSPECT ENGINE COMPRESSION • Inspect engine compression. (See COMPRESSION INSPECTION [L3].) • Is compression okay? | Yes | Go to next step.
No | Overhaul engine, then go to Step 11.
10 | INSPECT GENERATOR • Perform generator inspection. (See GENERATOR INSPECTION [L3].) • Is generator okay? | Yes | Go to next step.
No | Repair or replace related part, then go to next step.
11 | VERIFY TROUBLESHOOTING OF DTC P0506 COMPLETED • Make sure to reconnect all disconnected connectors. • Start engine. • Clear DTC from PCM memory using WDS or equivalent. • Depress brake pedal for 14.1 s or more.
• Is PENDING CODE of same DTC present?
Yes
Replace PCM, then go to next step.
(See PCM REMOVAL/INSTALLATION [L3].)
No | Go to next step.
12 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [L3].) • Is there any DTC present? | Yes | Go to applicable DTC troubleshooting. (See DTC TABLE [L3].)
No | Troubleshooting completed.