#
TORSION BEAM AXLE REMOVAL/INSTALLATION

BME021428320201

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.
  • Be careful when using the jack to avoid damaging the brake pipe and hose.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Brake caliper component
2 | Disc plate
3 | Hub cap
4 | Locknut (See Locknut Removal Note.) (See Locknut Installation Note.)
5 | Wheel hub and ABS sensor rotor
6 | Bolt
7 | Parking brake cable bracket
8 | Parking brake component
9 | Hub spindle
10 | ABS sensor harness bracket, ABS sensor and bolt (with ABS)
11 | Lateral rod (See Lateral Rod Removal Note.) (See Lateral Rod Installation Note.)
12 | Rear shock absorber (See REAR SHOCK ABSORBER AND SPRING REMOVAL/INSTALLATION.)
13 | Coil spring component (See REAR SHOCK ABSORBER AND SPRING REMOVAL/INSTALLATION.)
14 | Torsion beam axle (See Torsion Beam Axle Removal Note.)
15 | Trailing arm bushing (See Trailing Arm Bushing Removal Note.) (See Trailing Arm Bushing Installation Note.)

## Lateral Rod Removal Note

  Note

  • Jacking up the vehicle exerts force on the lateral rod, and makes it difficult to service. Lower the four wheels on the ground when servicing.

## Torsion Beam Axle Removal Note

1. Hold the center of the torsion beam axle using a jack.

2. Jack down the torsion beam axle gradually, and remove the torsion beam axle.

## Trailing Arm Bushing Removal Note

1. In order to set the installation position, mark the torsion beam axle in alignment with the small projection of the trailing arm bushing, as shown in the figure.

2. Press the trailing arm bushing out from the outer side of the trailing arm to the inner side using the SST.

## Trailing Arm Bushing Installation Note

1. Set the trailing arm bushing by aligning the small projection with the mark, as shown in the figure.

2. Press the trailing arm bushing in from the inner side of the trailing arm to the outer side using the SST.

## Lateral Rod Installation Note

1. Face the direction mark backward toward the outside of the vehicle, and install the lateral rod.