#
CYLINDER HEAD (II) DISASSEMBLY

B3E011002000214

1. Disassemble in the order indicated in the table.

1 | Engine hanger
2 | Valve keeper (See Valve Keeper Disassembly Note.)
3 | Upper valve spring seat
4 | Valve spring
5 | Valve
6 | Valve seal (See Valve Seal Disassembly Note.)
7 | EGR pipe
8 | Water outlet case

## Valve Keeper Disassembly Note

1. Remove the valve keeper using the SSTs.

When using the SST (49 JE02 0A2) (Europe only)

When using the SSTs (49 0636 100B, 49 B012 0A2)

## Valve Seal Disassembly Note

1. Remove the valve seal using the SST.