#
THIRD-ROW SEAT REMOVAL

BME09135730XW01

## TYPE A

1. Slide the seat to the rearmost position.

2. Pull the recliner lever and lower the seat back forward.

3. Lift and hold the seat-anchor bar and lift the entire seat up and forward.

4. Lift and hold the seat-anchor bar and lower the seat backwards a little to release it.

5. Remove the third-row seat.

## TYPE B

### Seat

1. Remove the bolts, and remove the third-row seat.

### Hinge

1. Remove the third-row seat.

2. Remove the rear side trim.

3. Remove the third-row seat belt lower anchor.

4. Remove in the order indicated in the table.

1 | Hinge cover
2 | Hinge

### Striker

1. Remove the rear side trim.

2. Remove the nuts, and remove the striker.