#
SECOND-ROW SEAT REMOVAL

BME09135720X201

## TYPE A

1. Slide the seat to the rearmost position.

2. Pull the recliner lever and lower the seat back forward.

3. Lift and hold the seat-anchor bar and lift the entire seat up and forward.

4. Lift and hold the seat-anchor bar and lower the seat backwards a little to release it.

5. Remove the second-row seat.

## TYPE B

1. Slide the seat to the rearmost position.

2. Remove the headrest.

3. Buckle insert seat cushion hole.

4. Pull the recliner lever and lower the seat back forward.

5. Lift and hold the lever and lift the entire seat up and forward.

6. Remove the long slider cover. (Left side seat only)

7. Remove the nuts

8. Remove the second-row seat.

## TYPE C

1. Place the buckle in the pocket in the cushion.

2. Slide the seat to the rearmost position.

3. Pull the recliner lever and lower the seat back forward.

4. Lift and hold the seat-anchor bar and lift the entire seat up and forward.

5. Remove the second-row seat.