#
NO. 3 TRANSMITTER ID CODE CANNOT BE REPROGRAMMED

BME090369000205

3 | Transmitter ID code cannot be reprogrammed
DESCRIPTION | • Malfunction in the transmitter battery, transmitter, door lock timer unit bracket, door lock timer unit bracket ground screw or door lock timer unit circuit
POSSIBLE CAUSE | • Malfunction in the transmitter battery, transmitter, door lock timer unit bracket, door lock timer unit bracket ground screw or door lock timer unit circuit

  - Transmitter battery, transmitter, door lock timer unit bracket, door lock timer unit bracket ground screw or door lock timer unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT TRANSMITTER BATTERY INSTALLATION AND TYPE • Visually inspect the transmitter battery. • Are below items okay?

  - Transmitter battery installation (correct polarity)
  - Battery type (CR2025 or CR1620)

Yes
Go to the next step.
No | Set the transmitter battery properly or replace with the specified transmitter battery (CR2025 or CR1620), then go to Step 8.
2 | INSPECT TRANSMITTER BATTERY TERMINALS FOR RUST AND POOR CONNECTION • Visually inspect the transmitter.

  - Is there rust on the transmitter battery terminals (positive or negative pole)?
  - Is there poor connection between the terminals and battery?

Yes
Replace the transmitter battery or repair the transmitter battery terminal, then go to Step 8.
No | Go to the next step.
3 | INSPECT TRANSMITTER BATTERY • Inspect the transmitter battery. • Is the battery voltage normal? | Yes | Go to the next step.
No | Replace the transmitter battery, then go to Step 8.
4 | INSPECT KEYLESS UNIT BRACKET INSTALLATION • Is the keyless unit bracket installed securely? | Yes | Go to the next step.
No | Install the bracket securely, then go back to Step 7 of keyless entry system preliminary inspection.
5 | INSPECT GROUND SCREW INSTALLATION BETWEEN KEYLESS UNIT AND KEYLESS UNIT BRACKET • Are the keyless unit and the keyless unit bracket installed securely by ground screw? | Yes | Go to the next step.
No | Install the screw securely, then go back to Step 7 of keyless entry system preliminary inspection.
6 | VERIFY WHETHER MALFUNCTION IS IN TRANSMITTER BATTERY OR ELSEWHERE • Replace with a known good transmitter battery. • Does keyless entry system operate properly? | Yes | Replace transmitter battery, then go to Step 8.
No | Go to the next step.
7 | VERIFY WHETHER MALFUNCTION IS IN TRANSMITTER OR KEYLESS UNIT • Reprogram transmitter ID codes using another known good transmitter. • Does keyless entry system operate okay? | Yes | Replace the transmitter and reprogram transmitter ID code, then go to the next step.
No | Replace the keyless unit and reprogram transmitter ID code, then go to the next step.
8 | RECHECK MALFUNCTION SYMPTOM AFTER REPAIR • Does keyless entry system operate properly? | Yes | Troubleshooting completed. Explain repairs to customer.
No | Recheck malfunction symptoms, then repeat from Step 1 if malfunction recurs.

  CR2025 :
European (L.H.D. U.K.) specs.
  CR1620 :
Australian and General (L.H.D. R.H.D.) specs.