#
FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION

BME091050031203

1. Disconnect the negative battery cable.

2. Remove the front bumper.(See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the headlight. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Support the radiator and the condenser using wire.

5. Remove the bolts.

6. Remove the bumper reinforcement.

7. Install in the reverse order of removal.