#
CLUTCH MASTER CYLINDER DISASSEMBLY/ASSEMBLY

BME051041990W04

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

G15M-R manual transaxle models

.

1 | Clip
2 | Hose
3 | Joint
4 | Bushing
5 | Snap ring (See Snap Ring Disassembly/Assembly Note.)
6 | Piston and secondary cap component
7 | Spacer
8 | Primary cap
9 | Return spring
10 | Bolt
11 | Gasket
12 | One-way valve piston
13 | One-way valve spring
14 | One-way valve pin
15 | Clutch master cylinder body

A65M-R manual transaxle models

.

1 | Clip
2 | Hose
3 | Joint
4 | Bushing
5 | Snap ring (See Snap Ring Disassembly/Assembly Note.)
6 | Piston and secondary cap component
7 | Spacer
8 | Primary cap
9 | Return spring
10 | Clutch master cylinder body

## Snap Ring Disassembly/Assembly Note

1. Hold the piston down using a cloth-wrapped pin punch.

  • If disassembling, remove the snap ring; if assembling, install it.