#
FUEL INJECTOR FUNCTION [MZR-CD (RF Turbo)]

BME011413250T01
• A small sized, energy saving, electromagnetically controlled injector has been adopted.
• A multiple fuel injection system has been adopted. The fuel injection amount and timing, as well as the division of the numerous injections are according to a PCM ON/OFF signal that controls the opening and closing of the electromagnetic valves.
• The construction and material of the electromagnetic valve has been modified to save energy and improve response.