#
BODY SHELL OUTLINE

BME091056100T01
• The floor of the vehicle is made flat to provide a more comfortable ride and to allow for multiple seating arrangements.
• To increase collision protection:

  - The frame is sectional (front, center, and rear) to distribute the impact.
  - Several crossmembers and torque boxes have been arranged laterally.
  - Construction has been designed to efficiently absorb and disperse impact forces.
  - Approximately half of the parts in the body shell are made of high-tensile steel for a lighter yet stronger body.
  - The front overhang has been reduced to improve vehicle maneuverability.