#
FRONT CONSOLE REMOVAL/INSTALLATION

BME091764270W01

1. Disconnect the negative battery cable.

2. Remove the lower panel.

3. Remove the glove compartment.

4. Remove the console lower cover.

5. Remove the screws.

6. Pull the front console toward you, then disengage clips A, B and pins C from the dashboard.

7. Disconnect the connector, and remove the front console.

8. Install in the reverse order of removal.