#
REAR AIRFLOW MODE ACTUATOR INSPECTION

BME074061070W02

1. Remove the rear airflow mode actuator.

2. Connect battery positive voltage to terminal F and ground to terminal G of the rear airflow mode actuator.

3. Connect ground to terminal A (B, C) of the rear airflow mode actuator.

4. Verify that the rear airflow mode actuator operates as shown below.

Terminal | Airflow mode
--- | ---
GND
A | HEAT
B | BI-LEVEL
C | VENT

5. Inspect for continuity between the rear airflow mode actuator terminals using an ohmmeter.

  • If not as specified, replace the rear airflow mode actuator.