#
NO.25 A/C DOES NOT CUT OFF UNDER WIDE OPEN THROTTLE CONDITIONS [AJ]

BME010300103230

25 | A/C does not cut off under wide open throttle conditions.
DESCRIPTION | • A/C compressor magnetic clutch does not disengage under wide open throttle.
POSSIBLE CAUSE | • TP sensor malfunction • TP sensor misadjustment • Loosely installed TP sensor

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Does the A/C compressor disengage when the A/C switch is turned off? | Yes | Go to the next step.
No | Go to symptom troubleshooting "No.24 A/C always on/ A/C compressor runs continuously". (See NO.24 A/C ALWAYS ON/A/C COMPRESSOR RUNS CONTINUOUSLY [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).)
(See NO.24 A/C ALWAYS ON/A/C COMPRESSOR RUNS CONTINUOUSLY [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
2 | • Connect the WDS or equivalent to the DLC-2. • Turn the ignition switch to the ON position (Engine off). • Retrieve any DTCs. • Is "PASSED" displayed? | Yes | No DTC is displayed: • Inspect the TP sensor for proper adjustment.
No | DTC is displayed: • Go to the applicable DTC inspection. (See DTC TABLE [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See DTC TABLE [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
3 | • Verify test results.

  - If normal, return to diagnostic index to service any additional symptoms.
  - If malfunction remains, inspect related Service Information and perform repair or diagnosis.

  • If vehicle is repaired, troubleshooting completed.
  • If vehicle is not repaired or additional diagnostic information is not available, replace or reprogram the PCM.