#
LIGHT SWITCH INSPECTION

BME091866121202

## L.H.D.

1. Remove the light switch.

2. Inspect for continuity between the light switch terminals using an ohmmeter.

  • If not as specified, replace the light switch.

Headlight switch

Turn switch

Front fog light / Rear fog light switch

Rear fog light switch

## R.H.D.

1. Remove the light switch.

2. Inspect for continuity between the light switch terminals using an ohmmeter.

  • If not as specified, replace the light switch.

Headlight switch

Turn switch

Front fog light / Rear fog light switch

Front fog light switch