#
INTERMEDIATE SENSOR INSPECTION [JA5A-EL]

BME051719200213

## On-Vehicle Inspection

1. Disconnect the terminal component No.2 connector.

2. Measure resistance between the terminals C and D.

  • If not within the specification, inspect the intermediate sensor. (See Individual Part Inspection.)

Resistance (ATF temperature: 20 °C {68 °F})

  513-627 ohms

3. Connect the terminal component No.2 connector.

## Individual Part Inspection

1. Remove the intermediate sensor. (See INTERMEDIATE SENSOR REMOVAL/INSTALLATION [JA5A-EL].)

2. Measure resistance between the terminals of the intermediate speed sensor.

  • If not within the specification, replace the intermediate sensor.
  • If it is normal, replace the harness.

Resistance (ATF temperature: 20 °C {68 °F})

  513-627 ohms

3. Install the intermediate sensor. (See INTERMEDIATE SENSOR REMOVAL/INSTALLATION [JA5A-EL].)