#
CYLINDER HEAD (I) ASSEMBLY

B3E011002000222

1. Assemble in the order indicated in the table.

1 | Water outlet case
2 | EGR pipe
3 | Valve seal (See Valve Seal Assembly Note)
4 | Valve
5 | Valve spring
6 | Upper valve spring seat
7 | Valve keeper (See Valve Keeper Assembly Note)
8 | Engine hanger

## Valve Seal Assembly Note

1. Press the valve seal onto the valve guide by hand.

2. Lightly tap the SST using a plastic hammer.

## Valve Keeper Assembly Note

1. Install the valve keeper using the SSTs.

When using the SST (49 JE02 0A2) (Europe only)

When using the SSTs (49 0636 100B, 49 B012 0A2)