#
DTC CLEARING PROCEDURE

BME090266900W03

1. Start the on-board diagnostic test mode.

2. First press the POWER button, then simultaneously press AUDIO CONT button for 2 seconds or more.

1 | POWER button (with RDS)
AUDIO CONT button (without RDS)
2 | AUDIO CONT button (with RDS)
POWER button (without RDS)

  Caution

  • Before clearing the DTCs, be sure to enter all of them displayed in the on-board diagnostic test mode in the Audio Repair Order Form.

3. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.