#
AFTER REPAIR PROCEDURE [FN4A-EL]

BME050201030203

  Caution

  • After repairing a malfunction, perform this procedure to verify that the malfunction has been corrected.
  • When this procedure is performed, be sure to drive the vehicle at lawful speed and pay attention to the other vehicles.

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the ignition switch to ON position (engine off).

3. Verify that DTCs are cleared from memory.

4. Decrease the ATF temperature to 20 °C {68 °F} or less.

5. Start the engine then wait 180 s or more.

6. Warm up the engine and ATX.

  • Engine coolant temperature: 60 °C {140 °F} or more.
  • Transaxle fluid temperature: 20 °C {68 °F} or more.

7. Shift the selector lever between the P position and the L range while depressing the brake pedal.

8. Drive the vehicle for 150 s or more at a vehicle speed between 25 and 59 km/h {15 and 36 mph}, then 60 km/h {37 mph} or more for 100 s or more.

9. Drive the vehicle in the D range and shift gears between 1GR and 4GR (TCC operation).

10. Gradually decelerate and stop the vehicle.

11. Make sure that the repaired DTC is not detected.