#
TROUBLESHOOTING INDEX

BME070301038202

No. | TROUBLESHOOTING ITEM | DESCRIPTION | PAGE
--- | --- | --- | ---
1 | Insufficient air (or no air) blows from front vents. | • Problem with each vent and/or duct. | (See NO.1 INSUFFICIENT AIR (OR NO AIR) BLOWS FROM FRONT VENTS)
2 | Amount of air blowing from front vents does not change. | • Malfunction in front blower system. | (See NO.2 AMOUNT OF AIR BLOWING FROM FRONT VENTS DOES NOT CHANGE)
3 | Airflow mode from front vents does not change. | • Malfunction in front A/C unit's airflow system. | (See NO.3 AIRFLOW MODE FROM FRONT VENTS DOES NOT CHANGE)
4 | Windshield fogs. | • Front climate control unit's FRESH indicator light does not illuminate while airflow is in DEFROSTER mode or HEAT/DEFROSTER mode. | (See NO.4 WINDSHIELD FOGS)
5 | No temperature control with front climate control unit | • Malfunction in front A/C unit's air mix system or heater piping. | (See NO.5 NO TEMPERATURE CONTROL WITH FRONT CLIMATE CONTROL UNIT)
6 | Insufficient air (or no air) blows from rear vents. | • Problem with each vent and/or each duct. | (See NO.6 INSUFFICIENT AIR (OR NO AIR) BLOWS FROM REAR VENTS)
7 | Amount of air blowing from rear vents does not change. | • Malfunction in rear blower system. | (See NO.7 AMOUNT OF AIR BLOWING FROM REAR VENTS DOES NOT CHANGE)
8 | Airflow mode from rear vents does not change. | • Malfunction in rear A/C unit's airflow system. | (See NO.8 AIRFLOW MODE FROM REAR VENTS DOES NOT CHANGE)
9 | No temperature control with rear climate control unit | • Malfunction in rear A/C unit's air mix system or heater piping. | (See NO.9 NO TEMPERATURE CONTROL WITH REAR CLIMATE CONTROL UNIT)
10 | Air from vent not cold enough | • Magnetic clutch operates but A/C system malfunctions. | (See NO.10 AIR FROM VENT NOT COLD ENOUGH)
11 | No cool air | • Magnetic clutch does not operate. | (See NO.11 NO COOL AIR)
12 | Noise while operating A/C system | • Noise from magnetic clutch, A/C compressor, hose or refrigerant line. | (See NO.12 NOISE WHILE OPERATING A/C SYSTEM)