#
PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L3]

BME011618740201

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Evaporative hose (to catch tank) (See Vacuum/Evaporative Hose Installation Note)
2 | Vacuum hose (to intake manifold) (See Vacuum/Evaporative Hose Installation Note)
3 | Purge solenoid valve

3. Install in the reverse order of removal.

## Vacuum/Evaporative Hose Installation Note

1. Fit the vacuum hose (purge solenoid valve) onto the respective fittings, and install clamps as shown.