#
TIMING CHAIN DISASSEMBLY

B3E011002000203

1. Disassemble in the order indicated in the table.

1 | Spark plug
2 | Cylinder head cover
3 | Crankshaft pulley lock bolt (See Crankshaft Pulley Lock Bolt Disassembly Note.)
4 | Crankshaft pulley
5 | Water pump pulley
6 | Drive belt idler pulley (Without stretch-type A/C drive belt)
7 | Engine front cover
8 | Front oil seal (See Front Oil Seal Disassembly Note.)
9 | Chain tensioner (See Chain Tensioner Disassembly Note.)
10 | Tensioner arm
11 | Chain guide
12 | Timing chain
13 | Seal (L3 (with variable valve timing mechanism))
14 | Oil pump chain tensioner
15 | Oil pump chain guide
16 | Oil pump sprocket (See Oil Pump Sprocket Disassembly Note.)
17 | Oil pump chain
18 | Crankshaft sprocket

## Crankshaft Pulley Lock Bolt Disassembly Note

1. Hold the crankshaft using the SST.

2. Remove the crankshaft pulley lock bolt.

## Front Oil Seal Disassembly Note

1. Remove the oil seal using a screwdriver.

## Chain Tensioner Disassembly Note

1. Hold the chain tensioner ratchet lock mechanism away from the ratchet stem with a thin screwdriver.

2. Slowly press the tensioner piston.

3. Hold the chain tensioner piston with a 1.5 mm {0.06 in} wire or paper clip.

## Oil Pump Sprocket Disassembly Note

1. Hold the oil pump sprocket using the SST.