#
FUEL PUMP (WATER HEATER SYSTEM) REMOVAL/INSTALLATION

BME074013350W01

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, do not damage the sealing surface of the fuel pump unit when removing or installing.

1. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

2. Disconnect the negative battery cable.

3. Remove in the order indicated in the table.

1 | Connector
2 | Fuel pump protector
3 | Fuel pump (water heater system)

4. Install in the reverse order of removal.

5. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].)