#
PCM FUNCTION DISPLAY OUTLINE [AJ]

BME014000000T78
• The driver can verify engine control information according to signals, outlined below, that the PCM sends to the instrument cluster.

## Fuel injection amount signal

• The fuel injection amount signal is sent in order to display instantaneous and average fuel economy on the driver information system display.

## Engine coolant temperature signal

• The PCM takes the signal from the engine coolant temperature sensor and sends it for display to the water temperature gauge.