#
LIFTGATE REMOVAL/INSTALLATION

BME091162010201

  Warning

  • Removing the stay damper without supporting the liftgate can be dangerous. The liftgate may fall and injure you. Open the liftgate fully and support it before removing the stay damper.

1. Disconnect the negative battery cable.

2. Remove the headliner.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Connector
2 | Rear washer hose
3 | Antenna plug
4 | Stay damper
5 | Liftgate (See LIFTGATE ADJUSTMENT.)
6 | Liftgate hinge