#
VALVE GUIDE REPLACEMENT

B3E011012111202

## Valve Guide Removal

1. Remove the valve guide from the combustion chamber side using the SST.

## Valve Guide Installation

1. Assemble the SSTs so that depth L is as specified.

Depth L:

  12.2-12.8 mm {0.481-0.501 in}

2. Tap the valve guide in from the side opposite the camshaft side until the SSTs contacts the cylinder head.

3. Verify that the valve guide projection height (dimension A) is within the specification.

Standard height:

  12.2-12.8 mm {0.481-0.501 in}