#
CLUTCH PEDAL POSITION (CPP) SWITCH INSPECTION [MZR-CD (RF Turbo) MTX]

BME014018660202

  Note

  • Perform the following test only when directed.

## Continuity Inspection

1. Inspect continuity between the clutch pedal position switch terminals using an ohmmeter.

  • If the clutch pedal position switch is normal, but the CPP PID is out of specification, perform the "Circuit Open/Short Inspection"
  • If not as specified, replace the clutch pedal position switch.

Specification

## Circuit Open/Short Inspection

1. Inspect for open/short circuit in the following wiring harnesses.

  • If there is open/short circuit, repair or replace wiring harnesses.

### Open circuit

  • Signal circuit
  - Clutch pedal position switch terminal C and PCM terminal 33
  • GND circuit
  - Clutch pedal position switch terminal E and GND

### Short circuit

  • Signal circuit
  - Clutch pedal position switch terminal C and PCM terminal 33 to GND.